This document details the installation instructions for the 
hardware drivers on the TeamPOS 2000 Retail POS Terminal for
the Windows 98SE operating system. 

 A. Preferred Order of Installation- To ensure no problems
    occur during the installation/updating of the hardware
    drivers for the TeamPOS 2000 a specified order of 
    installation is shown below. Please use this order of 
    installation when installing/updating the hardware 
    drivers.

  1. Video Driver
  a. The video driver has an extra installation instruction
     to assist customers with loading and  dual display
     operation. This should be the first driver updated. The
     Windows 98SE operating system does not have a video driver
     for the Chips 69030 video device. The driver from the download 
     set on this site must be used.
  
  
 2. Network Driver
  a. The Windows 98SE operating system does not install the
     proper network driver during installation. Instead Windows
     98SE will load the "Intel 8255x  driver." This should be
     updated with the approved driver found on this 
     website. The "Intel 82559 Fast Ethernet Lan on
     Motherboard" should be the adapter loaded in the Device
     Manager. 
     
 3. Audio Driver
  a. The Windows 98SE operating system does not have an audio 
     driver for the ESS Solo PCI audio device. The proper audio
     driver is located this website. After
     the audio driver is installed the volume icon may not show
     on the Windows task bar.  To fix this go into the Windows
     Control panel and click on the Multimedia icon. Remove and 
     replace the check mark next to the "Show Volume on taskbar" 
     entry and then click Apply. This should fix this issue.

 4. Touch Driver
  a. The touch driver should be downloaded from this website.
     A specific instruction is written to help with
     the various components of touch.
